R07922141

張緣彩

03/10/2018

Computer Vision Hw3 Report

Histogram Equalization

First calculate the frequency of each pixel (0~255). Then calculate sk according to the equation provided in the ppt. Finally, change every pixel from k to sk. The implementation is as below.

 

 

 